0.147u2
-------


MAMETesters Bugs Fixed
----------------------
- 05030: [DIP/Input] (coco3.c) coco3: Hi-Res joystick does not work for Tandy or CocoMax (sronco)
- 04878: [Crash/Freeze] (mac.c) macii and clones: Crash before OK with nb9 slot (R. Belmont)


Systems Promoted from GAME_NOT_WORKING:
---------------------------------------
- Macintosh LC [R. Belmont]
- Macintosh IIsi [R. Belmont]
- Macintosh LC II [R. Belmont]
- Macintosh Classic II [R. Belmont]
- Macintosh LC III [R. Belmont]
- Macintosh IIvx [R. Belmont]
- Macintosh IIvi [R. Belmont]


System Driver Changes:
----------------------
-snes.c: fixed Dezaemon SRAM mappings. [Fabio Priuli]

-gameboy.c: Added support for the mapper used by Sonic 3D Blast
5 pirate. [Wilbert Pol]

-samcoupe.c: modified the driver to not install / uninstall bank
handlers, greatly improving performaces (e.g. Manic Miner demo went
from 20% to 380% ingame). Plus added some very preliminary softlists.
[David Haywood]

-mac updates: [R. Belmont]
* Line-level ADB comms for machines using the Egret ADB MCU,
including standard transactions and SRQ
* Built-in video support for all modes on machines with the V8 and
Sonora ASICs
* Corrected some minor bugs in the ADB protocol spoken by the
keyboard simulation

-c128: Rewrote the driver using the PLA for address decoding.
[Curt Coder]

-gameboy.c: Partially implemented banking for Story of La Sa Ma.
[Wilbert Pol]

-mac: Support original Macintosh II Video Card
[R. Belmont, Sharkpuncher]

-hp9k: made drive go into boot process [Gabriele D'Antona]

-craft: added basic Timer 1 support to Craft driver and hooked up the DAC,
currently plays only a buzzing noise due to lacking EEPROM support
[MooglyGuy]

-mac: Convert 343-004x RTC/PRAM chip into modern RTC device
[R. Belmont]

-mac: Support headless operation [R. Belmont]

-mac updates: [R. Belmont]
* Fixed some glitches with the SE/30's built-in video
* Added preliminary infrastructure for LC and '030-type
processor-direct slots
* Support for SE/30 processor-direct slot version of RasterOps
Colorboard 264

-mac: Add support for Lapis ProColor Server 8*16 PDS video card
[R. Belmont, Sharkpuncher]

-mac: Add support for PDS Sigma Designs L-View card
[R. Belmont, Sharkpuncher]

-a2600: Reimplemented the a2600 controllers as vcs controller
devices. Switched the a2600 drivers to use slot devices for choosing
controllers. [Wilbert Pol]

-craft.c: Fixed DAC bit order, audio now plays but is 40% too slow
[Mooglyguy]

-craft.c: Preliminary video support, bad vsync and colors still.
[MooglyGuy]

-mac: Preliminary support for Micron XCEED 30HR and MacroColor
30 PDS cards [R. Belmont, Sharkpuncher, Balrog]

-a7800: NTSC Color Generator utilized for color palette with 
hue shift/start based on observation of several systems across 
multiple displays [Robert Tuccitto]

Software Lists:
----------------
-32x: added region compatibility filters to the software list
[Fabio Priuli, Tafoid, Bobz]

-spectrum_cass.xml: added very preliminary softlist containing
some interesting test case for emulation. [David Haywood]

-pcw16.xml: added softlist for available disk images [remax]

-snes.xml: added region compatibility filters to the software list
[Fabio Priuli, Tafoid, Bobz]

-amiga.xml: added placeholder lists for system disks. [David Haywood]

-amiga: added very preliminary softlist for game disks
[David Haywood]

-ibm5150.xml: updated with recent dumps. [Kaylee]

Source Changes
--------------
-floppy: Random fixes/logging [O. Galibert]

-upd765: Modernize [O. Galibert]

Remaining TODO list:
* take WP into account
* test the amstrad, implement its observational format (edsk) using
pasti as a start. Or find the legendary amstrad IPFs. Or both.
* correct read track, the implementation is completely wrong. See
previous for testing, it's only used in protections the check the
inter-sector gaps.
* shake and bake on the amstrad, protections are the best to find
bugs in a fdc
* add the scan id commands, but nothing seems to use them
* debug the 2.88M formatting which is unreliable. Fix its IDAM/DAM
gap size on formatting too (but that's not what's making it
unreliable)
* test all the systems that were hit, and fix what needs to be fixed.
Beware that multiple problems may happen:
* upd765 may be wrong
* the driver may not be working
* the hookup may be wrong/incomplete (bitrate selection and floppy
rpm in particular)
* the driver may be too limited for the new implementation (the x68k
dma device does not handle non-instant dma yet for instance)
* report invalid command when appropriate depending on the actual
chip emulated
* add the russian clones with their real names

-d88: Reduce the gap3 size from the standard value when the data
otherwise won't fit [O. Galibert]

-upd765: Implement LOCK [O. Galibert]

-upd765: Fix busy status when seeking [O. Galibert]

-upd765: Fix MSR DIO in EXEC phase [O. Galibert]

-add innovation ssi-2001 sid-on-isa device [Carl]

-upd765: Fix the dump regs command, don't exit on unknown
commands and add dsr reset [O. Galibert]

-added basic support for the loop flags in tzx [David Haywood]