# MAME/MESS keymap for Portuguese QWERTY 105-keys keyboard (Linux)
# SDL can tell the difference between the two COMPOSE keys but assigns them the same label
# thus both CLOSEBRACE and BACKSLASH appear like "´ ~" in the user interface.
# The following definitions are therefore correct.
#
# Row 1
#
ITEM_ID_TILDE      SDLK_BACKSLASH 0x31 0x5c \
ITEM_ID_MINUS      SDLK_QUOTE     0x14 0x27 '
ITEM_ID_EQUALS     SDLK_WORLD_11  0x15 0xab «
#
# Row 2
#
ITEM_ID_OPENBRACE  SDLK_PLUS      0x22 0x2b +
ITEM_ID_CLOSEBRACE SDLK_COMPOSE   0x23 0x00 ´
#
# Row 3
#
ITEM_ID_COLON      SDLK_WORLD_71  0x2f 0xe7 Ç
ITEM_ID_QUOTE      SDLK_WORLD_26  0x30 0xba º
ITEM_ID_BACKSLASH  SDLK_COMPOSE   0x33 0x00 ~
#
# Row 4
#
ITEM_ID_BACKSLASH2 SDLK_LESS      0x5e 0x3c <
ITEM_ID_SLASH      SDLK_MINUS     0x3d 0x2d -
#
# Row 5
#
ITEM_ID_RALT       SDLK_MODE      0x71 0x00 ALTGR