0.144u5

New System Drivers Supported:
-----------------------------
- Palm Z22 [Tim Schuerewegen]
- Mini2440 [Tim Schuerewegen]
- Mera-Elzab Meritum I (model 2) [Miodrag Milanovic]
- RM-380Z [Gabriele D'Antona]

Systems Promoted from GAME_NOT_WORKING:
---------------------------------------
- SLC1 [Robbbert]

Skeleton drivers:
-----------------
- Axel AX-20
- Didaktik M 92
- Mera 79152PC
- Mera Konin
- Siemens PC-D [rfka01]
- NCR Decision Mate V [rfka01]
- DEC Rainbow 100B [rfka01]

System Driver Changes:
----------------------
-poly1: Added Terminal roms [Andrew Trotman]
-Fix for a400, a800 and clones which caused a crash navigating the Input menu.  [hap]
-a5105: Implemented memory banking. [Sandro Ronco]
-mac: Cuda device talks to the 680x0 properly; Color Classic now shows something. [R. Belmont]
-mac: Fixed Cuda timer interrupt ack and default PRAM for Egret and Cuda [R. Belmont]
-victor9k: Fixed keyboard MCU clock. [Lord Nightmare]
-nc: Added v1.02 Danish and v1.02 German bios variations
 of the NC100.  [Roberto Carlos Fernandez Gerhardt]
-cbm: Added ICT Mini Chief hard disk ROMs. [Curt Coder]
-mac: add preliminary support for LC520 (not working yet) [R. Belmont]
-pet: Added skeleton for SSE SoftBox IEEE-488 peripheral. [Curt Coder]
-macpci: new driver to support PCI-based Old World Macs, including Pippin [R. Belmont]
-c64: Added skeleton for Serial Box IEC peripheral. [Curt Coder]
-mac: Added skeleton device for low-level emulation of the original Mac keyboard [R. Belmont]
-ip22: Made the SGI Indy driver about 130% faster on my machine (from 50% speed to 115% speed on a 3.2GHz i7)
 by commenting out debug logging wholesale rather than leaving in an inline do-nothing if(). [MooglyGuy]

Software Lists:
----------------
-coleco.xml: added an earlier dump of dkong. [k1w1]
-rainbow.xml: DEC Rainbow 100 Softlist [Kaylee]

Source Changes:
----------------
-pc_cga.c: Fixed selection of mc6845 input clock.  [Wilbert Pol]
-floppy: Add media type and write splice information to the internal 
 representation, and start handling HD [O. Galibert]
-8530scc: Modernize.  Hopefully nothing broke [O. Galibert]
-floppy: Add an "unknown" form factor and use it to fix floptool [O. Galibert]
-mcs48: Fixed I8021/I8022 clock divider. [Curt Coder]
-i386: Patch for i386 helps booting Phoenix bios [Carl]
-scsibus: Increment command index on acknowledge instead of data read, 
 since Visual 1050 BIOS skips the message byte read and just acks it. [Curt Coder]
-Fix four spc700 opcodes which didn't disassemble correctly [kevtris]
-scsibus: Added group 6 (vendor specific) command length. [Curt Coder]
-scsibus: Implemented SASI group 6 command 00 (C0, Physical Device ID). [Curt Coder]
-scsibus: Sector size is now configurable in init_scsibus. [Curt Coder]
-scsihd: Get sector size from CHD metadata to support old 256 bytes/sector 
 SASI drives, and allow hard disk image subdevices. [Curt Coder]
-uiimage/diimage: Dumbify the menus and add a control layer [O. Galibert]
-floppy: Add diskferret format support, and a minimal pc support [O. Galibert]
-First draft of i8279 device. Hooked up to mmd2, which now nearly works [Robbbert]
-softlist: Fix entry count tracking issue [O. Galibert]